***************************************************************************************

Project Name		SmartPSS
Version			V1.11.0
Base Platform		V1.10.0
Operation Platform	10.7 or above

New Function
    1.  Video can save bit stream type of video window
    2.  New Smart Search function
    3.  Alarm link video stream type can be set
    4.  Alarm supports event record playback
    5.  Support for M30 device

Revised Function
    1.  TV wall config interface is changed to include mixed layout
    2.  PC-NVR may choose disk size allocation
    3.  Complete authorization for alarm link, device configuration
    4.  Fix problem of device login when there are multiple devices
    5.  Sync playback, problem of async playback progress in different channels are solved
    6.  For device with three streams£¬problem of main/sub stream switch under preview is solved
    7.  NVR6000 and EVS5000£¬not bound remote channel by order, and cannot open preview, playback channel in disorder
    8.  Problem of TV wall task configuration file not copied during config path change is solved
    9.  Digital zoom, pane select IPC device, fixed problem of blurred screen
    10. Fixed other bugs


***************************************************************************************

Project Name		SmartPSS
Version			V1.10.0
Date			2014/05/24
Base Platform		V1.00.5
Operation Platform	10.7 or above

New Function
    1.   Add navigation button
    2.   Add custom window split
    3.   Add view function, may save one preview mode
    4.   Window scale includes full-screen and original size
    5.   Add preview-to-playback switch function and device configuration 
    6.   Drag device to other group
    7.   Add area zoom in and PTZ mouse stimulation function
    8.   Add event playback mode
    9.   Add search record function under view mode
    10.  New module£¬may search system log, operation log, alarm log and device log, and support export
    11.  Add device list order function
    12.  Add device online/offline status display
    13.  Add collation of disk allocation

Revised Function
    1.   Group creation is moved under preview tree
    2.   PTZ display is moved under device tree
    3.   Advanced speed dome preset, tour setup intersection
    4.   Advanced virtual rocker control£¨speed dome PTZ and fish eye E-PTZ£©
    5.   Record export by time is changed to cut mode
    6.   Search record by time supports up to 24-hour period
    7.   Revise problem of one-hour time difference on record caused by DST
    8.   Advanced record search, and long-time waiting caused by network problem, may cancel search task
    9.   Auto search device interface is moved into device configuration homepage, and support double click to add device
    10.  In device configuration homepage, buttons of device config and channel config will change as device or channel is selected in device tree
    11.  Consistent style of device config pages
    12.  Revised alarm config page
    13.  Modified tour adding method
    14.  Video preview in tour config, user-friendly scheme adding
    15.	 PC-NVR can only add one at once
    16.  PC-NVR remote channel binding method is changed
    17.  PC-NVR record plan configuration interface is changed
	
Deleted Function
    1.   Delete local resource management module, and function is moved to local playback function
    2.   Delete alarm link module from homepage£¬and function is combined into alarm list management
    3.   Delete PC-NVR config function
    4.   Delete device config entrance in device management
    5.   Delete group config in device management
